# 

The drilling will be carried out through a rigid one-part capsule equipped with an adhesive foam ensuring its fixing on the floor or the wall and of a centering guiding the drill through a gel collecting the dust emissions (such as SAFE'CAP, manufactured by Gerflor).